**Extension Mobility**

Cisco Extension Mobility (EM) allows you to temporarily configure a Cisco Unified IP Phone as your own. After you sign in to EM, the phone adopts your user profile, including your phone lines, features, established services, and web-based settings. Your system administrator sets up EM for you.

**Enable Extension Mobility**

**Procedure**

|  |  |
| --- | --- |
| **Step 1** | Press the **Applications** button <https://www.cisco.com/c/dam/en/us/td/i/200001-300000/250001-260000/255001-256000/255310.eps/_jcr_content/renditions/255310.jpg>. |
| **Step 2** | Select **Extension Mobility**. (Use the Navigation bar and button to scroll and select.) |
| **Step 3** | Enter your user ID and PIN (Default PIN 0987). |
| **Step 4** | To log out, press the **Application**s button. |
| **Step 5** | Select **Extension Mobility.** |
| **Step 6** | When prompted to log out, press the **Yes** soft key. |

**Extension Mobility**

Η φορητότητα επέκτασης Cisco (EM) σας επιτρέπει να ρυθμίσετε προσωρινά ένα ενοποιημένο IP τηλέφωνο Cisco ως δικό σας. Αφού εισέλθετε σε EM, το τηλέφωνο υιοθετεί το προφίλ χρήστη σας, συμπεριλαμβανομένων των τηλεφωνικών γραμμών, των δυνατοτήτων, των εγκατεστημένων υπηρεσιών και ρυθμίσεων.

**Ενεργοποίηση φορητότητας επέκτασης**

**Διαδικασία**

|  |  |
| --- | --- |
| **Βήμα 1** | Πατήστε το κουμπί **Applications**  <https://www.cisco.com/c/dam/en/us/td/i/200001-300000/250001-260000/255001-256000/255310.eps/_jcr_content/renditions/255310.jpg>. |
| **Βήμα 2** | |  | | --- | | Επιλέξτε **Extension Mobility**. (Χρησιμοποιήστε τη γραμμή περιήγησης και το κουμπί για κύλιση και επιλογή.) | |
| **Βήμα 3** | Εισαγάγετε το user ID και το PIN (προεπιλεγμένο PIN 0987). |
| **Βήμα 4** | Για να αποσυνδεθείτε, πατήστε το κουμπί **Application**s. |
| **Βήμα 5** | Επιλέξτε **Extension Mobility.** |
| **Βήμα 6** | Όταν σας ζητηθεί να αποσυνδεθείτε, πατήστε το πλήκτρο **Ναι.** |